AOpen/DX34 BIOS REVISION
Date	BIOS Version	Release Notice	CheckSum		
08/09/00	(E0) R1.00	1. M25D/AO R00.07
2.  Fixed key +/- is abnormal in setup
3.  DX34 model ID : E0h 
    DX34 Plus model ID : D6h	8100h		
08/31/00	R1.00 01	Base from DX34Plus R1.01 02	8F00h		
09/07/00	R1.01	1. Fixed Multi-ECC cannot log issue
2. Fixed system will hung up when lm80 & i2cbuffer event is generated 
3. Fixed system hung up 00h when AC Power is removed at cp 23h
4. Some Raid (sub-class is I2O) always last boot issue
5. Fixed boot sequence menu abnormal issue in setup menu
	B600h		
09/14/00	R1.02	1. Added some code to prevent that DIMM2, DIMM3 ECC error will log DIMM1 issue
2. Fixed windows whistler cannot insatall issue
3. Change LM80 threshold value <added>
4. Fixed System Temp Event, it can log multi times now 	B500h		
09/19/00	R1.02  01	1. Fixed Power cycle function abnormal issue when Action after Critical Event--[Power Cycle] 
2. Change CPU voltage threshold value 	C100h		
09/20/00	R1.02  02	1. Fixed DMI table Type 10 abnormal issue 
2. Change CPU Fan event format (Please use Elview after V1.04.01) 	AD00h		
09/22/00	R1.02  03	1. Support Power Supply Redudant Event	C300h		
09/22/00	R1.02  04	1. Change AGP buffer strength for ECh to CCh when system use AGP 4X Card 
2. AGP Fast Write [Enabled] -> [Disabled] 	C300h		
09/26/00	R1.02  05	1. Change CPU thermal threshold value	0200h		
09/27/00	0925-1.02  06	1. Remove PCI event log & Memory ECC event Log   	4400h		
09/27/00	0925-1.02  07	1. Remove critical process items in setup menu	3200h		
10/02/00	0925-R1.03	1. Based form DX34 R1.02 07 
2. Fixed Floppy LED always on issue with 1GB CPU and HTC Boot DISK
3. Mass Production	3400h	Formal Release
53.50F01.031	
10/03/00	R1.03 01	1. Don't INIT VIA H/W Monitor	DE00h		
10/09/00	R1.03 04	1. Disabled EX_SMI during system enter S1
2. Update RASII BIOS 2.0 001003
=> Change CPU thermal threshold value	BC00h		
10/12/00	R1.04	1. Don't INIT VIA H/W Monitor
2. Disabled EX_SMI during system enter S1 
3. declare I/O port CA0h in ACPI ASL code
4. Fixed DPT FDD issue
5. Update RASII BIOS 2.0 001003
   => Change CPU thermal threshold value	DD00h		
10/30/00	R1.03 05	1. Don't INIT VIA H/W Monitor
 2. Added I/O Port CA0h in ACPI motherboard resource
 3. Added I/O APIC Memory Map IO FEC00000h~FEC00FFFh in ACPI motherboard resource
 4. Added Local APIC Memory Map IO FEE00000h~FEE00FFFh in ACPI motherboard resource	E600h		
10/30/00	R1.03 06	1. Fixed APM32 Entry is overlay issue	0F00h		
11/15/00	R1.04 00	1. Support Win98 
=> Don't INIT VIA H/W Monitor
=> Added I/O Port CA0h in ACPI motherboard resource
=> Added I/O APIC Memory Map IO FEC00000h~FEC00FFFh in ACPI motherboard resource
=> Added Local APIC Memory Map IO FEE00000h~FEE00FFFh in ACPI motherboard resource
2. Fixed APM32 Entry is overlay issue
3. Change ACPI Feature 
=> Disabled EX_SMI during system enter S1
=> Fixed PS2 Mouse cannot use in w2k/win98 when ps2 kb don't connect
=> Fixed sometimes PS2 KB/Mouse cannot use in W2K when USB Legacy [Enabled]
=>Add Operation of OS Type FLAG for ACPI for Solaris 8 cannot use floppy issue
4. Fixed SCO OPEN Server 5.0.5 cannot use floppy with DPT Card 
5. Change DRAM Refresh Counter(VT694X Device0 RX6Ah) Algorithm 
6. BIOS Setup Menu Debug
 => If "PCI IRQ setting" item is set [Auto], ignore PCI Slots setting,	then "IDE controller" still can select [Disable/Primary/Both]    
 => Fixed System information PS2 Mouse always show Install issue when  PS/2 Mouse Controller--[Enabled]
 => Fixed setup "boot option" issue
7. Fixed Resume Day on RTC Alarm is ignored 
8. Update RASII BIOS 2.0 001006
   => Change CPU thermal threshold value
	7B00h		
11/16/00	R1.04 01	1. Fixed MP table is overlay issue	AB00h		
12/07/00	R1.04 02	1. Fixed dummy PCI Device issue (Bus0 Device4 Fun04)	AB00h		
12/22/00	R1.04 03	1. Fixed added-on Adaptec 39160 SCSI Card can not find 2nd SCSI hard disk issue	AC00h		
02/09/2001	R1.05	=>Added Mux168A01.TXT for PIII D0-Stepping CPU
=>Fixed WinMe will wakeup immediately after system enter S4.	6C00h		
03/08/2001	R1.06	1. Support HYUNDAI 128MB DIMM*3 
2. Change CPU VID information in DMI Table
       Real VID     DMI Table
         1.6v 	=>  1.6v
         1.65v	=>  1.6v
         1.7v 	=>  1.7v 
         1.75v	=>  1.7v	4F00h		
03/28/2001	R1.10	1. Support new flashrom SST39SF040
2. Support new BIOS Password Spec
3. Change CMOS default Setting
     Memory ECC Mode --- [Disabled]	E300h	Formal Release
53.50F01.032	
05/07/2001	R1.11	1. Added setup item "USB Host Controller" in PnP/PCI option
2. update mu168314.txt for PIII B0-Step	FC00h