United States

Compaq Presario Internet PC 7000 Series Computers | SPECIFICATIONS

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

CD OR DVD DRIVE/ CD-RW DRIVE DISK DRIVE FAX/ MODEM POWER SUPPLY ASSEMBLY SYSTEM BOARD | Fax/Modem
Fax/Modem
General Description |
Support | Supports K56flex and/or ITU-T V.90. 14400bps send and receive fax modem with automatic fallback to 12000, 9600, 7200, 4800, and 2400bps.
| Supports fax service Class 1 (EIA/TIA 578). Supports V.80 video ready modem. Built-in DTE interface with speed up to 115.2kbps or 57.6kbps, parallel 16550a UART-compatible interface. Power Management Registers to PCI Interface.
Data Mode | K56flex and/or ITU-T V.90 56kbits/s for highest Internet connection rates. Ultrahigh compression throughput due to parallel access directly to the host PC. ITU-T V.34 extended rates 33600bps to 2400bps. V.32terbo, V.32bis and fallbacks. TIA/EIA 602 standard for AT command set. V.42 error correction (LAM and MNP). V.42bis and MNP Class 5 data compression.
Fax Mode | Fax modem send and receive rates up to 14400bps. * V.17, V.29, V.27ter, and V.21 channel 2 * TIA/EIA 578 Class 1 FAX
Error Correction | ITU-T recommended V.42 error correction. V.42 error correction (LAM and MNP).