United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Removing the Memory Modules and Continuity Modules (continued)
| Removal Press out and downward on the release latches found at each end of the memory module and continuity modules . Lift the memory modules and continuity modules from the memory slots . The number of memory modules may vary depending upon your system's configuration. Replacement Ensure that the latches at each end of the memory modules are released. Align the memory modules and continuity modules with the memory slots. Push the memory modules and continuity modules carefully and firmly into the slot, ensuring that the latches on both ends snap into place.
NOTE | The blank modules in RIMM slots 3 and 4 must be removed and replaced on the new system board.
IMPORTANT | The memory slots on the system board are labeled RIMM1, RIMM2, RIMM3, and RIMM4. Look closely at the base of the memory slot connector by the release latches for the slot number.