United States

Compaq Presario Internet PC 7000 Series Computers | PRODUCT DESCRIPTION

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

MODELS AND FEATURES CPU CONTROLS AND LIGHTS SIDE ACCESS PANEL INTERNET KEYBOARD CONTROLS REAR CPU CONNECTORS POWER CORD SET REQUIREMENTS |  | Power Cord Set Requirements
Requirements: The power cord set (flexible cord and wall plug) received with the computer meets the requirements for use in the country where the computer was purchased. Power cord sets for use in other countries must meet the requirements of the country where you use the computer. For more information on power cord set requirements, contact your Compaq authorized dealer, reseller, or service provider. General Requirements: The requirements listed below are applicable to all countries: The length of the power cord set must be at least 6.00 feet (1.8 m) and a maximum of 9.75 feet (3.0 m). All power cord sets must be approved by an acceptable accredited agency responsible for evaluation in the country where the power cord set will be used. The power cord set must have a minimum current capacity of 10A and a nominal voltage rating of 125 or 250 Volts AC, as required by each country's power system. The appliance coupler must meet the mechanical configuration of an EN 60 320.IEC 320 Standard Sheet C13 connector, for mating with the appliance inlet on the Switch Box. Country-Specific Requirements:
Country | Accredited Agency
United States | UL*
US/Canada | UL and CSA
| * The flexible cord must be Type SJT-2 or equivalent, No. 18 AWG, 3-conductor. The wall plug must be a two-pole grounding type with the NEMA 5-15P (15A, 125V) or NEMA 6-15P (15A, 250V) configuration.