United States

Compaq Presario Internet PC 7000 Series Computers | SPECIFICATIONS

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

CD OR DVD DRIVE/ CD-RW DRIVE DISK DRIVE FAX/ MODEM POWER SUPPLY ASSEMBLY SYSTEM BOARD | CD or DVD Drive/ CD-RW Drive Please select a drive to view specifications: CD Drive DVD Drive CD-RW Drive
CD Drive
Dimensions | U.S. | Metric
Width | 5.75 in | 15.01 cm (maximum)
Height | 1.67 in | 4.29 cm
Depth | 8.23 in | 20.80 cm
Weight | 2.65 lb | 1.200 kg
Modes Supported |  |
CD-ROM | Mode 1 and Mode 2 |
CD-DA | Audio |
CD-XA | Mode 2, Form 1 and 2 |
Photo CD | Multiple Session |
Video-CDI | Multiple Session |
CD-Plus/CD-Extra/CD Enhanced | Multiple Sesssion |
CD-RW | Multiple Session |
Block Size |  |
CD-ROM Mode 1 and Mode 2 Form 1 (XA) | 2048 bytes |
CD-ROM Mode 2 | 2336 bytes |
CD-DA | 2324 bytes |
CD-XA | 2324 bytes |
Center Hole | 1.5 mm diameter |
Diameter | 120 mm/80mm |
Thickness | 1.2mm |
Track Pitch | 1.6mm |
Laser |  |
Divergence Angle | 53.5 degrees +/- 1.5 degrees |
Output Power | 0.14 mW (@ objective lens) |
Type | Semiconductor laser GaAIAs |
Wave Length | 780nm +/- 25 nm |
Access Time |  |
Random | < 100 ms (typical) |
Full Stroke | < 150 ms (typical) |
Audio Output Level |  |
Line Out | 0.7 Vrms ±20% |
Headphone | 0.6 Vrms ±20% |
Cache Buffer | 256 KB |
Data Transfer Rate |  |
| Mode 1 | Mode 2
Sustained | 4800 KB/sec | 5475 KB/sec
| KB.sec (32x) | KB/sec (32x)
Burst | MB/sec | MB/sec
Startup Time | < 5 sec |
Stop Time | < 5 sec |
Return to top
DVD Drive
Dimensions | U.S. | Metric
Width | 5.75 in | 15.01 cm (maximum)
Height | 1.67 in | 4.29 cm
Depth | 8.23 in | 20.80 cm
Weight | 1.80 lb | 0.90 kg
Modes Supported | Mode 1 and Mode 2 |
Block Size | 2048 bytes |
Center Hole | 15 mm diameter |
Disc Diameter | 12 cm, 8 cm |
Thickness | 1.2 mm |
Track Pitch | 10.74 µm |
Access Time |  |
Random | <180 ms typical |
Full Stroke | < 300 ms |
Audio Output Level |  |
Line Out | 1.0 V (RMS) at 47 kW |
Headphone | 0.7 V (RMS) at 32 W |
Cache Buffer | 512 Kb |
Data Transfer Rate |  |
Sustained | 2705-8115 KB/sec |
Burst |  |
Startup Time | < 10 sec |
Stop Time | < 2 sec |
Return to top
CD-RW Drive
Dimensions | U.S. | Metric
Width | 5.75 in | 15.01 cm (maximum)
Height | 1.67 in | 4.29 cm
Depth | 8.23 in | 20.80 cm
Weight | 2.65 lb | 1.200 kg
Modes Supported |  |
CD-ROM | Mode 1 and Mode 2 |
CD-DA | Audio |
CD-XA | Mode 2, Form 1 and 2 |
Photo CD | Multiple Session |
Video-CDI | Multiple Session |
CD-Plus/CD-Extra/CD | Multiple Session |
Enhanced |  |
CD-RW | Multiple Session |
Block Size |  |
CD-ROM | 2048 bytes |
Mode 1 and Mode 2 Form 1 (XA) |  |
CD-ROM Mode 2 | 2336 bytes |
CD-DA | 2324 bytes |
CD-XA | 2324 bytes |
Center HOle | 1.5 mm diameter |
Diameter | 120 mm/80mm |
Thickness | 1.2 mm |
Track Pitch | 1.6mm |
Access Time |  |
Random | < 95 ms |
Full Stroke | < 190 ms |
Audio Output Level |  |
Line Out | 0.7 Vrms ±20% |
Headphone | 0.6 Vrms ±20% |
Cache Buffer | 256 KB |
Data Transfer Rate |  |
| Mode 1 | Mode 2
Sustained | 4800 KB/sec | 5475 KB/sec
| KB/sec (32x) | KB/sec (32x)
Burst | MB/sec | MB/sec
Startup Time | < 5 sec |
Stop Time | < 5 sec |
Return to top