United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Removing the 1394 Card, continued
| Removal Remove the screw from the 1394 card. Using a gentle rocking (side-to-side) motion, pull the 1394 card from the PCI slot on the system board. Replacement Align the 1394 card with the PCI slot on the system board and with the expansion card rear connector. Insert the card carefully and firmly into the slot. Replace the screw to secure the 1394 card to the chassis. Reconnect the 1394 data and power cable from the Front I/O bracket to the connector on the 1394 card.
IMPORTANT | During replacement, the 1394 card rear connector must be properly inserted into the rear chassis slot to ensure the card is properly seated into the connector on the system board.