United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Removing the Graphics Card, continued
| Removal Remove the screw securing the graphics card. Push the locking tab on the AGP slot away from the graphics card to release . Using a gentle rocking motion, pull the unlocked graphics card from the AGP slot on the system board . Replacement Align the graphics card with AGP slot on the system board. Pull the locking tab on the AGP slot, and insert the card carefully and firmly into the connector. Release the locking tab to lock the graphics card into the AGP slot. Replace the screw securing the graphics card to the chassis.