United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Removing the System Board, continued
| Removal Remove the Microprocessor/ Heatsink Assembly: Identify the Microprocessor/ Heatsink Assembly. This illustration identifies the microprocessor/ heatsink assembly clips , heatsink with a fan , heatsink fan power cable , microprocessor , heatsink brackets , interface socket with a lever . Next Step
NOTE | Depending on the model selected, tape may be used for shipping.
IMPORTANT | The microprocessor/ heatsink assembly may vary depending on your computer's configuration.