United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Preparation for Disassembly To prepare the computer for removal and replacement procedures, complete the following steps: Remove any disk or compact disc from the computer. Turn off the computer and any peripheral devices that are connected to the computer.
| CAUTION
| The computer power switch should be turned off before you disconnect any cables.
| CAUTION
| Before doing any work inside your computer, ground yourself by touching a metal part of the chassis.
Disconnect the power cord from the electrical outlet, and then from the computer.
| WARNING
| Failure to disconnect the power from the computer may result in personal injury.
Disconnect all peripheral device cables from the computer. Turn the computer over on its side (open side facing up).
IMPORTANT | During disassembly, label each cable as you remove it. Be sure to note its position and routing.