United States

Compaq Presario Internet PC 7000 Series Computers | SPECIFICATIONS

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

CD OR DVD DRIVE/ CD-RW DRIVE DISK DRIVE FAX/ MODEM POWER SUPPLY ASSEMBLY SYSTEM BOARD | Power Supply Assembly
Power Supply Assembly
Input Specifications | U.S.
Nominal Line Voltage | 115 to 230 VAC
Range Input Line | 90 to 264 VAC
Frequency Range | 47 to 63 Hz AC
Input Current | 115V 3.00 AMPS
Input Current | 4.5 RMS at Max Load
Output Power | 145 Watts
Inrush Current | 80 A at 132 VAC (cold start)
Holdup Time | 16 ms from zero
Environment | Temperature Range
Operating | 10 to +50 C
Non-Operating | -40 to +66 C