United States

Compaq Presario Internet PC 7000 Series Computers | REMOVAL AND REPLACEMENT PROCEDURES

PRODUCT DESCRIPTION | TROUBLESHOOTING | ILLUSTRATED PARTS CATALOG
REMOVAL AND REPLACEMENT PROCEDURES | JUMPER AND SWITCH INFORMATION | SPECIFICATIONS

ELECTROSTATIC DISCHARGE SERVICE CONSIDERATIONS PREPARATION FOR DISASSEMBLY SERIAL NUMBER SIDE ACCESS PANEL GRAPHICS CARD EXPANSION CARD (Modem or Network Card) SOUND CARD 1394 CARD MEMORY MODULE HARD DRIVE DISK DRIVE REMOVING THE TOP DOOR REMOVING THE CD STORAGE DOOR (Lower Front Panel - Open the CD Storage Door) OPTICAL AND MASS STORAGE DEVICES (CD, CD-RW and/or DVD Drive, Hard Drive, Disk Drive) FAN ASSEMBLY POWER SUPPLY ASSEMBLY FRONT I/O BOARD SYSTEM BOARD COMPONENTS (RTC Battery, Microprocessor/Heatsink Assembly) | Removing the Microprocessor/Heatsink Assembly, continued
| Removal Push down, pull out, and lift the lever which secures the microprocessor inside the microprocessor interface socket, and remove the microprocessor . Replacement
NOTE | A small tab secures the lever . You might push down and pull out before lifting it.