ACY-25 System / Keyboard BIOS Release Check List	

System Configuration		Date: 10/09/2002
CPU:		Intel Pentiun 4, 1.5 GHz	Operation System:	Windows XP Pro   (Build 2600)	
L2 Cache:	256 KB	System/EC BIOS:	1.08 / K12X108	
RAM Size:	Apacer 128 MB	M/B Rev.:	C	
HDD:	IBM IC25N020ATCS04-0	Battery:	8-cell	
DVD-ROM:	TOSHIBA SD-C2502	Mini PCI Card:	Modem (Askey)	
Panel:	LG LP150x04	Tested By:	Serene Hsy/Tracy Hsieh	

	OS & Driver Installation		PASS		FAIL	
		Issue No.		
01.			Clean Install Windows XP Professional manually from ODD	v		
03.			Update SiS Graphics driver (v6.13.10.2081 (logo’d))	v		
04.			Update Realtek Audio driver (v5.10.0.3850 (logo’d))	v		
05.			Update Alps TouchPad driver (v5.3.203.3 (logo’d))	v		
06.			Realtek Network driver (v5.502.131.2002 (logo’d))		(native)		
07.			Update Askey Modem driver (v3.1.113.0 (logo’d))	v		
08.			Update PCMCIA INF (v5.1.2600.1001 (logo’d))	v		
09.			Update PCMCIA ATA Patch (v1.04)	v		
10.			Update 802.11b (v1.7.37.0 (logo’d))	v		
11.			Install WinDVD 3.1	v		
	Power Management Test (single loop)	
01.			Suspend.exe - S3	v		
02.			Lid - None (Turn off panel only)	v		
03.			Lid – Standby	v		
04.			Lid – Hibernate	v		
05.			Power Button – Standby	v		
06.		Power Button – Hibernate	v		
07.			Power Button – Shutdown	v		
08.			Power Button - 4-Second Override	v		
09.			Time-out Turn off monitor	v		
10.			Time-out Standby	v		
11.		Time-out Hibernate	v		
12.		SpeedStep	v		
	I/O Port and Built-in Devices Test (Without S1/S3/S4 PM Transition)	
01.			Parallel Port (HP DeskJet 930c)	v		
02.			Serial Port (Mouse)	v		
03.			USB keyboard legacy-free support	v		
04.			USB Port (left) (Microsoft IntelliMouse Explorer)	v		
05.			USB Port (Microsoft IntelliMouse Explorer)	v		
06.			USB Port (next to 1394) (Microsoft IntelliMouse Explorer)	v		
07.			PCMCIA Lagacy Card	v		
08.			PCMCIA CardBus Card	v		
09.			PCMCIA ATA Card (Billionton CF Adapter + SanDisk Card)	v		
10.			TV-Out	v		
11.			Mic-In	v		
12.			Headphone	v		
13.		 	Mini-PCI Modem: Dialer Dial test	v		
14.		 	Mini-PCI Modem: Hyper Terminal Dial test	v		
15.			Mini-PCI Modem: Hyper Terminal WOR test	v			
16.			Internal TouchPad (click, drag, scroll up, scroll down)	v		
17.		 	Internal Keyboard (key-press, hot key, ctrl-alt-del, F2, ESC)	v		
18.			Built-in LAN	v		
19.			PXE	v		
20.			Built-in 1394 (HDD)	v		
Other Basic Functional Test (Without S1/S3/S4 PM Transition)	
01.			Check all Status LED working.	v		 	
02.	 	Check all Control Buttons working	v	 	
03.			Media Player AVI Playback	v			
04.			Power DVD - DVD Playback	v		

MDP Test 	
01.		PASS 	Boot time  	38.81
38.52
38.83
38.24
39.70
38.56		 	
02.		PASS 	Standby Resume time  		3.48
3.40
3.18
3.37
3.46
3.50	 	
03.		PASS 	Hibernate Resume time  		17.30
	17.31
	17.18
	17.14
	17.31
	17.21		 	

			Fix Issue No.		System BIOS Release Note (Solve Issues) Check List		PASS		FAIL	
01.			Fixed system can't show current Cache size during POST	v		
02.			Fixed system hang on debug code "B9" when panel ID DIPswitch was 0xFh.	v		
03.			Implement Flash LOGO ROM using Flash Utility.	v		
04.			Set reserved panel ID to force CRT only	v		
05.			Fixed LCD display garbage when setting TV-OUT under WinXP on CPT SXGA+ panel	v		

			Fix Issue No.		EC BIOS Release Note (Solve Issues) Check List		PASS		FAIL	
01.			Update PS2 code for function for resume from S3 lock up issue		v			

Comments: